Practical Report

# Overview

# Design

* Considered doing a nested struct for flags, however this was not used as with only 3 flags (each uint8\_t) it was hard to pad
* TODO: Byte order?
* Repeated timeout on FIN. What happens? Back off?
* RST?

Diagram

Description automatically generated

# Testing

# Evaluation/Issues

# Conclusion